= decklink-debugger

A tool to probe all inputs of all Blackmagicdesign DeckLink cards in a Linux system, detecting if a signal is present and which image-format it has, showing the results on the terminal and via HTTP on port 8042, allow capturing still images.

== Building

See the GitHub project page for instructions how to build the software.

== Supported devices

The devices need to support auto configuration. The following list shows which devices are known to be supported by decklink-debugger. Feel free to add new devices to it.

Name	Recognized	Auto detection works	Tested by
Decklink HD Pro	✔	✘	TheAssassin
Intensity Pro	✔	✘	sophie
Decklink Mini Recorder 4k	✔	✔	sophie
Decklink MiniRecorder	✔	✔	MaZderMind
Decklink Duo 2	✔	✔	MaZderMind