Infobeamer on 38C3

We have one device for each lecture hall. In addition, we run two more devices in the VOC office to present content on the various displays located elsewhere in CCH.

Running your own

We allow attendees and other interested persons to run their own info-beamer pis to show information about stuff happening at their assembly/location. C3VOC can not provide you with a display nor a raspberry pi.

If you want to run a pi, please follow these instructions:

Get a monitor (atleast 1920×1080), a raspberry pi (atleast 2B), a matching SD card (atleast 4GB) and a matching power supply

Download the info-beamer install image

install.img.gz (Gzipped Disk Image, 64MB) - SHA256 804c82b12ee11ed6e93e4c0c58052737a03b76b23684fac8a32166688236c7cc

install.img (Disk Image, 72MB) - SHA256 d37b1b2a9cf3d9d1a3d77dd67b5a5eb59882c0d2f5d9601bc8e7340230dfb62f

Flash the .img to the sd card (unzipping it first if needed)

The image will only use wired ethernet. If you require WiFi connectivity, please configure that according to the info-beamer documentation.

Insert the SD card into the raspberry pi, connect monitor and ethernet cable, then connect power to the pi.

The device will now boot up, initialize the sd card and get added to our account.

Wait until the screen shows a test card and your devices serial number

Contact us using our IRC Channel #infobeamer on irc.hackint.org (also bridged to matrix) or #info-beamer on the cccv rocketchat instance. We will need the following information

Contact information (DECT/E-Mail/Matrix preferred)

Device serial number as shown on screen

Name of your assembly/room/whatever (or UUID, if you know it) - Please explicitely tell us if you don't want your device assigned to an assembly

Do not use E-Mail to contact us. Do not query people hanging out in IRC.

An operator will configure the device according to your request. Please stay in IRC until your request has been acknowledged.