Panasonic AG-AC 160 AEJ

datasheet

Audio XLR input

XLR (3-pin) x 2 (AUDIO INPUT1, AUDIO INPUT2)

LINE/MIC selectable, high impedance

LINE: 0 dBu (for more about dBu see 1 2 )

MIC: -40/-50/-60 dBu (menu selectable)

MIC POWER +48 V ON/OFF switchable

Pegel in dBu	Spannung in Volt
Studiopegel ARD	+6	1,550
Studiopegel USA	+4	1,228
Normpegel 1 V	+2,22	1
Normpegel 0,775 V	0 Bezug	0,775
Heimtechnik	−7,78	0,316
-40	0.00774
-50	0.00245
-60	0.00077

out: HDMI (only in HD mode), SDI, DV (only in SD mode)

resolutions:

Progressive mode

so we don't need to deinterlace manually using 1080 with HD-SDI

Camera Manual Part 2, Page 23:

You can shoot in progressive mode when you select 25P for 1080 mode in AVCHD mode or 25P for 576 mode in DV mode in the REC FORMAT item on the setup menu RECORDING SETUP screen. […]

25P mode: Shoots 25 frames/second in the progressive mode.For output and recording of video signal, the 25 frames/second image is converted to 50-field-per-second interlace signal [for SDI output]. This mode gives high quality video.

Audio

Settings:

Limiter

The limiter is a compressor with a threshold off 0db or a little below 0 an 0ms attack and 1:∞ compression.The limiter is disabled when the the pegel switch is set to “AUTO”