= Flight Cases This page aims to provide an overview on our flight cases. For details on the content of the cases follow the links below or the Hardware namespace startpage.

== Lecture Room Case (S1 to S6) Currently we have four cases of generation 1 and two of generation 2. They should include everything needed in the lecture rooms. Each part is either labeled or color coded with a cable tie. The current state and constant differences are listed at Hardware status.

Room 1: Green

Room 2: Yellow

Room 3: Blue

Room 4: Red

Room 5: Black

Room 6: White

Wie man den Spanngurt richtig am VOC-Case befestigt

Together with an Audio-Case and an Auer-Box (often shipped together) the weight per room set is ~100-140kg)

=== S1 to S4

A single first generation case is (incl. wheels) 102cm wide, 72cm high and has a depth of 54cm. Height without wheels is 57cm.

Content list of the room cases with more photos

=== S5 + S6

Note: Hardware of S6 was migrated into Case 2.0 Prototype and now consists of two flight cases.

Content list of 2nd generation room cases

==== Measurements A single second generation case is (incl. wheels) 104cm wide, 72cm high and has a depth of 54cm.

Height without wheels is 59cm.

==== Spare parts

Wheels: 100mm caster worked well and should be replaced in pairs (eg. Millenium Blue Wheel MkII)

== Audio cases (A1, A2, A3, A4, A5, A6)

Content of the audio case

LxBxH: 55 x 55 x 40 cm

== Regie Box (R1): SDI over Fibre

LxBxH: 60x40x20 cm (Auer-Box)

Contains:

3x Meshbag Blackmagic Fibre, each containing 2 each Netzteil BM, BM Converter, SDI BNC Module.

Various Fibres

== Regie Box (R2): Office

LxBxH: 60x40x32 cm (Auer-Box)

Contains various items to build a voc office:

Ethernet Switch

Ethernet Cables

Schuko Cables and extensions

Various kinds of tape

Phone

USB-HDD

…

See wink for details.

== hacc racc (H): hackers against climate change rack

hacc video streaming rack, loosely modeled after standard voc case.

LxBxH: 83x55x90 cm