Epiphan Broadcaster

We have three VGA Broadcaster light (old generation, no longer available) and two VGADVI Broadcaster from Epiphan. Despite their names both can handle DVI and VGA.

Dimensions 202×105×35 mm

VGA Broadcaster light

We have three VGA Broadcaster light (old generation, no longer available) and two VGADVI Broadcaster from Epiphan. Despite their names both can handle DVI and VGA. Calls itsself “VGA Broadcaster Davinci”. Part of in room case 2, 3 & 4.

Manual epiphan_vga_broadcaster_lite_user_guide.pdf

To clear any frame grabber adjustments (FPGA only), delete the value from one or more fields and select Apply. To have changes take effect, you must reboot the VGA Broadcaster Lite device. You can make more than one change before selecting 'Apply' and rebooting.

Settings:

MJPEG with “Default” setting (not “High speed”)

25 fps, quality 50-70

Frame Size: 1280×720 (otherwise high latency, see note above)

no audio

no recording

VGADVI Broadcaster

Part of in room case 1 & 5

Manual: epiphan_3_11_vgadvi-broadcaster-userguide.pdf

Settings:

MJPEG with “High speed”

25 fps, quality 50-70

no recording

Operating the Framegrabber

See here.

hax0r

broadcaster lite partition layout

Disk /dev/sdc: 1967 MB, 1967128576 bytes
61 heads, 62 sectors/track, 1015 cylinders, total 3842048 sectors
Units = sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 512 bytes
I/O size (minimum/optimal): 512 bytes / 512 bytes
Disk identifier: 0x00000000
Device Boot Start End Blocks Id System
/dev/sdc1 * 1 1051395 525697+ b W95 FAT32
/dev/sdc2 * 1051396 3838729 1393667 83 Linux