VGA Broadcaster light

Calls itsself “VGA Broadcaster Davinci”. Used in Rooms 2, 3 & 4.

Manual epiphan_vga_broadcaster_lite_user_guide.pdf

To clear any frame grabber adjustments (FPGA only), delete the value from one or more fields and select Apply. To have changes take effect, you must reboot the VGA Broadcaster Lite device. You can make more than one change before selecting 'Apply' and rebooting.

Settings:

MJPEG with “Default” setting (not “High speed”)

25 fps, quality 50-70

Frame Size: 1280×720 (otherwise high latency, see note above)

no audio

no recording

VGADVI Broadcaster

Used in Room 1 & 5

Manual: epiphan_3_11_vgadvi-broadcaster-userguide.pdf

Settings:

MJPEG with “High speed”

25 fps, quality 50-70

no recording

Operating the Framegrabber

See here.