Epiphan Broadcaster

We have three VGA Broadcaster light (old generation, no longer available) and two VGADVI Broadcaster from Epiphan. Despite their names both can handle DVI and VGA.

Dimensions 202×105×35 mm

VGA Broadcaster light

We have three VGA Broadcaster light (old generation, no longer available) and two VGADVI Broadcaster from Epiphan. Despite their names both can handle DVI and VGA. Calls itsself “VGA Broadcaster Davinci”. Part of in room case 2, 3 & 4.

Manual epiphan_vga_broadcaster_lite_user_guide.pdf

To clear any frame grabber adjustments (FPGA only), delete the value from one or more fields and select Apply. To have changes take effect, you must reboot the VGA Broadcaster Lite device. You can make more than one change before selecting 'Apply' and rebooting.

Settings:

MJPEG with “Default” setting (not “High speed”)

25 fps, quality 50-70

Frame Size: 1280×720 (otherwise high latency, see note above)

no audio

no recording

VGADVI Broadcaster

Part of in room case 1 & 5

Manual: epiphan_3_11_vgadvi-broadcaster-userguide.pdf

Settings:

MJPEG with “High speed”

25 fps, quality 50-70

no recording

Operating the Framegrabber

See here.