= Cameras: JVC GY-HM200E

JVC product page

manual

brochure

== notes default password 0000

== specs

Single 1/2.3-inch CMOS image sensor w/12.4M pixels

High quality integrated 12x F1.2-3.5 zoom lens (35mm equivalent: 29.6-355mm)

Dynamic Zoom in HD mode combines optical zoom and pixel mapping to create seamless and lossless 24x zoom

4K Ultra HD recording (150 Mbps) to SDHC/SDXC (UHS-I Speed class 3) cards

4:2:2 Full HD (24-60p) recording at 50Mbps

Live 4K UHD output via HDMI connector

HD-SDI (3G)

Advanced JVC streaming engine compatible with c3voc

2-channel XLR audio inputs with phantom power

IP Network Remote Control, Remote Viewing, Metadata editing, FTP clips

2 position ND filter (1/4, 1/16)

Built-in stereo microphone

Dual SDHC/SDXC slots enable dual backup & continuous recording

3.5-inch colour LCD display (920K pixel) w/smart focus assist

Wired remote control supported

HDMI output (4K output via HDMI only)

0.24-inch colour viewfinder (1.56M pixel) with smart focus assist function

9 user button assignable functions

Includes handle unit, SSL-JVC50 7.4V battery and AC adapter

== things we tested

RTMP 1080p stream from cam to enginx RTMP / Voctomix

HD SDI 1080p

1080p / 4k record to card

== API

curl 'http://10.73.6.9/cgi-bin/cmd.cgi'
-XPOST
-H 'Content-Type: application/x-www-form-urlencoded; charset=UTF-8'
-H 'X-Requested-With: XMLHttpRequest'
–data '{“Request”:{“Command”:“GetCamStatus”,“SessionID”:“5ec39adc641a52612745f96bd7c53c48”}}'

{
"Response": {
"Requested": "GetCamStatus",
"Result": "Success",
"Data": {
"Status": "Rec",
"Mode": "Camera",
"RecMode": "Normal",
"ZoomStatus": "Off",
"ZoomDynamicPos": "328",
"ZoomPosition": "106",
"TC": "06:24:26:06",
"SlotA": {
"Status": "SelectRec",
"Protect": "Unlock",
"Remain": "316",
"ClipNum": 1,
"RemainWarn": 0
},
"SlotB": {
"Status": "NoSelect",
"Protect": "Unlock",
"Remain": "708",
"ClipNum": 0,
"RemainWarn": 0
},
"Battery": {"Info": "Time", "Level": "1", "Value": "0" },
[…]
"Fullauto": "Off",
"Iris": {"Status": "Auto", "Letter": "AF5.6"},
"Gain": {"Status": "ManualL", "Letter": " 0dB"},
"AeLevel": {"Adjust": "Off", "Status": "AeOn", "Letter": " ±0"},
"Shutter": {"Status": "Step", "Letter": " 1/50 "},
"Whb": {
"Status": "Preset",
"Letter": "P< 5600K>",
"WhPaintRScale": 64,
"WhPaintBScale": 64,
"WhPaintRPosition": 32,
"WhPaintBPosition": 32,
"WhPaintRLetter": " ",
"WhPaintBLetter": " "
},
"Focus": {"Status": "MF", "Letter": " 19m"},
[…]
}
}
}