Cameras: JVC GY-HM200E

JVC product page

manual

brochure

== notesdefault password 0000

specs

Single 1/2.3-inch CMOS image sensor w/12.4M pixels

High quality integrated 12x F1.2-3.5 zoom lens (35mm equivalent: 29.6-355mm)

Dynamic Zoom in HD mode combines optical zoom and pixel mapping to create seamless and lossless 24x zoom

4K Ultra HD recording (150 Mbps) to SDHC/SDXC (UHS-I Speed class 3) cards

4:2:2 Full HD (24-60p) recording at 50Mbps

Live 4K UHD output via HDMI connector

HD-SDI (3G)

Advanced JVC streaming engine compatible with c3voc

2-channel XLR audio inputs with phantom power

IP Network Remote Control, Remote Viewing, Metadata editing, FTP clips

2 position ND filter (1/4, 1/16)

Built-in stereo microphone

Dual SDHC/SDXC slots enable dual backup & continuous recording

3.5-inch colour LCD display (920K pixel) w/smart focus assist

Wired remote control supported

HDMI output (4K output via HDMI only)

0.24-inch colour viewfinder (1.56M pixel) with smart focus assist function

9 user button assignable functions

Includes handle unit, SSL-JVC50 7.4V battery and AC adapter

things we tested

RTMP 1080p stream from cam to enginx RTMP / Voctomix

HD SDI 1080p

1080p / 4k record to card

== API

curl 'http://10.73.6.9/cgi-bin/cmd.cgi' \

XPOST \

H 'Content-Type: application/x-www-form-urlencoded; charset=UTF-8' \

H 'X-Requested-With: XMLHttpRequest' \

-data '{“Request”:{“Command”:“GetCamStatus”,“SessionID”:“5ec39adc641a52612745f96bd7c53c48”}}'

<code javascript>{ “Response”: { “Requested”: “GetCamStatus”, “Result”: “Success”, “Data”: { “Status”: “Rec”, “Mode”: “Camera”, “RecMode”: “Normal”, “ZoomStatus”: “Off”, “ZoomDynamicPos”: “328”, “ZoomPosition”: “106”, “TC”: “06:24:26:06”, “SlotA”: { “Status”: “SelectRec”, “Protect”: “Unlock”, “Remain”: “316”, “ClipNum”: 1, “RemainWarn”: 0 }, “SlotB”: { “Status”: “NoSelect”, “Protect”: “Unlock”, “Remain”: “708”, “ClipNum”: 0, “RemainWarn”: 0 }, “Battery”: {“Info”: “Time”, “Level”: “1”, “Value”: “0” }, […] “Fullauto”: “Off”, “Iris”: {“Status”: “Auto”, “Letter”: “AF5.6”}, “Gain”: {“Status”: “ManualL”, “Letter”: “ 0dB”}, “AeLevel”: {“Adjust”: “Off”, “Status”: “AeOn”, “Letter”: “ ±0”}, “Shutter”: {“Status”: “Step”, “Letter”: “ 1/50 ”}, “Whb”: { “Status”: “Preset”, “Letter”: “P< 5600K>”, “WhPaintRScale”: 64, “WhPaintBScale”: 64, “WhPaintRPosition”: 32, “WhPaintBPosition”: 32, “WhPaintRLetter”: “ ”, “WhPaintBLetter”: “ ” }, “Focus”: {“Status”: “MF”, “Letter”: “ 19m”}, […] } }}</code>