Mini Converter UpDownCross HD

https://www.blackmagicdesign.com/products/miniconverters/techspecs/W-CONM-28

Connections

SDI Video Inputs

1 x SD, HD or 3G‑SDI Video Input and 1 x External Reference Input.

HDMI Video Input

1 x HDMI type A connector.

SDI Video Outputs

1 x loop out and 2 x outputs

HDMI Video Output

HDMI type A out. Output supports EDID of the monitor.

SDI Rates

270Mb, 1.5G, 3G.

Reference Input

Black burst and Tri‑Sync for SD & HD.

Multi Rate Support

Auto detection of HD or standard definition SDI inputs.

Reclocking Yes

StandardsSD Video Standards525i59.94 NTSC, 625i50 PAL

HD Video Standards720p50, 720p59.94, 720p60, 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60, 1080PsF23.98, 1080PsF24, 1080PsF25, 1080PsF29.97, 1080PsF30, 1080i50, 1080i59.94, 1080i60

HDMI Input Video Standards720p50, 720p59.94, 720p60, 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60, 1080i50, 1080i59.94, 1080i60

SDI ComplianceSMPTE 259M, SMPTE 292M, SMPTE 296M, SMPTE 424M‑B, ITU‑R BT.656 and ITU‑R BT.601.

SDI Metadata SupportTimecode and closed captioning.

SDI Video RatesSDI video connections are switchable between standard definition and high definition.

SDI Video Sampling4:2:2

SDI Audio SamplingTelevision standard sample rate of 48 kHz and 24 bit.

SDI Color Precision4:2:2

SDI Color SpaceYUV

SDI Auto SwitchingAutomatically detects SD, HD or 3G‑SDI.

Format ConversionVideo ConversionConvert any SD and HD input to “720p50, 720p59.94, 720p60, 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60, 1080i50, 1080i59.94, 1080i60”

Computer ScalingScale DVI resolutions 640×480, 800×600, 1024×768 to 525i59.94, 625i50,720p50, 720p59.94, 720p60 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60 1080i50, 1080i59.94, 1080i60