Mini Converter UpDownCross HD

https://www.blackmagicdesign.com/products/miniconverters/techspecs/W-CONM-28

Connections

** SDI Video Inputs *** 1 x SD, HD or 3G‑SDI Video Input and 1 x External Reference Input. ** HDMI Video Input *** 1 x HDMI type A connector. ** SDI Video Outputs *** 1 x loop out and 2 x outputs ** HDMI Video Output *** HDMI type A out. Output supports EDID of the monitor.

SDI Rates

** 270Mb, 1.5G, 3G.

Reference Input

** Black burst and Tri‑Sync for SD & HD.

Multi Rate Support

** Auto detection of HD or standard definition SDI inputs. *Reclocking Yes

Standards SD Video Standards 525i59.94 NTSC, 625i50 PAL

HD Video Standards 720p50, 720p59.94, 720p60, 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60, 1080PsF23.98, 1080PsF24, 1080PsF25, 1080PsF29.97, 1080PsF30, 1080i50, 1080i59.94, 1080i60

HDMI Input Video Standards 720p50, 720p59.94, 720p60, 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60, 1080i50, 1080i59.94, 1080i60

SDI Compliance SMPTE 259M, SMPTE 292M, SMPTE 296M, SMPTE 424M‑B, ITU‑R BT.656 and ITU‑R BT.601.

SDI Metadata Support Timecode and closed captioning.

SDI Video Rates SDI video connections are switchable between standard definition and high definition.

SDI Video Sampling 4:2:2

SDI Audio Sampling Television standard sample rate of 48 kHz and 24 bit.

SDI Color Precision 4:2:2

SDI Color Space YUV

SDI Auto Switching Automatically detects SD, HD or 3G‑SDI.

Format Conversion Video Conversion Convert any SD and HD input to “720p50, 720p59.94, 720p60, 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60, 1080i50, 1080i59.94, 1080i60”

Computer Scaling Scale DVI resolutions 640×480, 800×600, 1024×768 to 525i59.94, 625i50,720p50, 720p59.94, 720p60 1080p23.98, 1080p24, 1080p25, 1080p29.97, 1080p30, 1080p50, 1080p59.94, 1080p60 1080i50, 1080i59.94, 1080i60