Reencoder

Te be able to provide video streams to all clients from iPhone to Linux desktops we provideour streams in different resolutions, containers and codecs.

Services:

Transcoding

Remote encoding worker

Speedy & Tweedy

Speedy and Tweedy are to machines build into one 1HE case.

1x Travla T1220

2x Intel Core i7 6700K, 4x 4.00GHz, So.1151, TRAY (CM8066201919901)

2x ASRock Z170M-ITX/ac - Motherboard - Mini-ITX - LGA1151 Socket

2x Corsair Value Select 8GB PC4-17000 - 8 GB - DDR4 - 2133 MHz

2x HGST Ultrastar 7K3000 HUA723020ALA641 - Festplatte - 2TB -

2x Dynatron DYN Kühler K-199 A 1HE

2x Seagate Samsung SpinPoint M9T ST2000LM003 - Festplatte - 2TB -

=== Deployment

Reset and start

Wake up Speedy:

ssh ber.c3voc.de 'sudo sispmctl -o 1' && ssh root@wrt254.lan.c3voc.de 'etherwake -i br-lan d0:50:99:84:00:fb'

Wake up Tweety:

ssh ber.c3voc.de 'sudo sispmctl -o 2 && ssh root@wrt254.lan.c3voc.de 'etherwake -i br-lan d0:50:99:83:fe:cc'

Hard-Reset Speedy:

ssh ber.c3voc.de 'sudo sispmctl -f 1; sudo sispmctl -o 1'

Hard-Reset Tweety:

ssh ber.c3voc.de 'sudo sispmctl -f 2; sudo sispmctl -o 2'

Additional BIOS settings

activate Advanced configuration

ACPI Configuration → PCI Devices Power On

Power on failure → enabled