Sony PXW-Z200

Settings

Project:

Rec Format:

Frequency: 25

Codec: XAVC S, S-L420

Video format: 1920

Quality: Low

Bit Rate: 16M

Simul Rec:

Setting: Off

Proxy Rec:

Setting: On

Proxy Format: 1920P 16

Audio Channel: CH1/CH2

Chunk: 2min

Monitoring:

Display On/Off:

Enabled are: Network Status, File Transfer, Rec/Play Status, Focus Mode, Focus Position, Focus Area Ind., Subject Recognition Frame, Tacking AF Pointer, Zoom Position, Digital Extender, TODO

Marker:

Setting: On

Color: White

Center Marker: Off

Safety Zone: Off

Aspect Marker: Mask

Aspect Mask: 6

Aspect Safety Zone: Off

Aspect Select: Custom

Custom Aspect Ratio: 09.00:14:00

Guide Frame: Off

100% Marker: Off

User Box: Off

Zebra:

Setting: Zebra2

Zebra1 Level: 70%

Zebra1 Aperture: 10%

Zebra2 Level: 100%

Audio:

Audio Input:

CH1 Input Select: INPUT1

CH2 Input Select: INPUT2

{CH3,CH4} Input Select: Internal MIC

{INPUT1,INPUT2} MIC Reference: -50dB

Line Input Reference: -3dB

Reference Level: -20dB

{CH1,CH2} Wind Filter: Off

{CH3,CH4} Wind Filter: On

{CH3,CH4} Level Control: Auto

{CH3,CH4} Input Level: 49

Audio Input Level: 90

CH1&CH2 AGC Mode: Stereo

CH3&CH4 AGC Mode: Stereo

AGC Spec: -6dB

{CH1,CH2} Level: Level+Side

{CH3,CH4} Level: {CH3,CH4} Input Level

Network:

File Transfer:

Auto Upload: On

Auto Upload (Proxy): Chunk

Default Upload Server: VOC Storage

Server Settings 1:

Service: FTP

Host Name: storage.lan.c3voc.de

Port: 21

User Name: saal${num}-sony, PW see BW “./scripts/passwords-for storage”

Passive Mode: Off

Destination Directory: S${num}

Using Secure Protocol: Off

Note: With the “Audio Input Level” set to 90 and the side rotary dials set to 10, an output of +10 dB of the CQ18-T will barely clip the input.This should be a safe level when aiming for a 0dB output level.