Captures EDID information from a display and presents it to a computer. Useful in situations where the DDC lines are not connected (like the CCH).

website https://github.com/datenwolf/vgaedidinjector

Persons working on: Datenwolf

The VGA EDID Injector is a tool that aims to make the use of presentation infrastructure less painful. In many conference venues the presentation displays (video projectors aka “beamers”) are connected using old fashioned analogue connections using high quality coax cable. While this method offers a very good image quality it suffers from the lack of a DDC channel for transmission of EDID data.

Modern operating systems however depend on the EDID information for mode setting. Even worse on some operating systems it is very hard or even impossible to override the settings obtained from the EDID data. Those operating systems also usually fall back to a set of safe display resolutions and timings if no EDID data could be retrieved via DDC. Unfortunately those safe timings usually don't match the physical resolution of the display device, resulting in bad looking scaling and/or worse distortion of the aspect ratio (e.g. fall back resolution 1024×768 (4:3 aspect), display device physical resolution 1280×720 (16:9) resulting in squashed image, i.e. pancake heads, and so on…).

The VGA EDID Injector provides relief for this kind of situation: It allows to take a snapshot of a display's EDID information and “carry” it to the computer in need.

Hardware

The VGA EDID Injector has 3 connectors (see image):

D-Sub 15 H (VGA) female, left side of the board – connect to display device

D-Sub 15 H (VGA) male, right side of the board – connect to computer

Micro-USB, lower side of the board – for providing auxiliary power (+5V); upcoming firmware revisions will provide a command line interface

Usage

Snapshoting Display EDID information

Connect the display to the left side, female VGA connector.Plug the right side, male VGA connector into a computerUsing the display control tools refresh/identify connected displays. Repeat this until the attached display is recognized.The VGA EDID Injector can now be spliced into the computer side of a video signal only (i.e. no DDC signals) connection.

Replaying snapshoted EDID information

Simply insert the VGA EDID Injector into the video signal connection close to the computer.

Important Notice: There must be no DDC signals present on the display side of the connection. Otherwise the VGA EDID Injector will try to attempt to snapshot the information found there and, if successful, will overwrite the previously snapshoted EDID information.

In that case it is recommended to prepare a special VGA cable in which the signal carried over the pins 12 and 15 is severed (simply removing the pins from one of the connectors with some side cutters and/or pliers will do the trick).

Micro-USB connector

An upcoming firmware release will provide a command line interface over USB CDC ACM serial device emulation. Until then the Micro-USB connector serves for supplying auxiliary power (+5V). Under normal circumstances the VGA connection will provide +5V, 50mA(max) over pin 9. However long cable lengths or a “weak” system's power supply (think laptops) may prevent the supply to meet the demands.

The circuitry of the VGA EDID Injector incorporates two rectifier diodes to prevent current to flow back into either the VGA port or the Micro-USB if both are connected at the same time, or should a computer get accidently connected on the display side. However those diodes create a 0.7V voltage drop.

Hence should the VGA EDID Injector seem to be nonoperational it is suggested to provide auxiliary power through the Micro-USB connector.

(copy from https://web.archive.org/web/20140708233324/https://events.ccc.de/congress/2013/wiki/Projects:VGA_EDID_Injector )