zido x8 and x9s

Vendor website x8 http://www.zidoo.tv/Product/index/model/X8/target/WhrwiBL1anZKKmVViAFMcQ%3D%3D.html x9s http://www.zidoo.tv/Product/index/model/X9S/target/rRwtRFydZ4xKKmVViAFMcQ%3D%3D.html

SoC – Realtek RTD1295DD

System Memory – 2GB DDR3

Storage – 8GB (x8) / 16GB (x9s) eMMC flash + micro SD slot + SATA 3.0 (x9s only)

Video Output / Input – HDMI2.0a output up to 4K, HDMI input with PVR and Time Shifting support (up to 1080p), and AV port (Composite + stereo audio)

Audio I/O – HDMI Out and In, AV, and optical S/PDIF

Connectivity – 10/100/1000M Ethernet, 802.11ac Wi-Fi, Bluetooth 4.0

USB – 1x USB 3.0, 2x USB 2.0 host ports.

Misc – ON/OFF switch, IR receiver

Android 6

== As a ethernet stream source=== instreamer

The instreamer app allows to stream the HDMI input via Ethernet / wifi to a stream sink

https://github.com/robbi5/instreamer

To be able to use instreamer, an ffmpeg binary compiled for the ARM CPU needs to be placed in /mnt/sdcard. Such an binary can be found e.g. at https://github.com/WritingMinds/ffmpeg-android/releases

After the first launch, press Menu for the Settings. This is the ffmpeg command that already worked on the Tronsmart Pavo M9:

ffmpeg -i - -c copy -absf aac_adtstoasc -f flv rtmp://100.122.3.243:1935/source/tronsmart