Setting up a room

This page will only offer the basics. If you need specialized setups (like, for example, embedding audio into the HDMI signal) please get in touch with an experienced voc person if you don't know what you're doing.

We assume we have received the following from the venue:

a desk for speakers to put their laptop on

a desk for us to put the mixer laptop and the audio mixer on

a projector with a cable long enough to reach to the speaker desk

at least one loudspeaker, ideally with enough cable to reach the audio mixer

a network port which we can use to

Some more in german

Platzierung der Hardware:

Hörsaal o.ä. (Audio und Beamer vorne):

Kamera, Mixer-Laptop, Encoder und Audio an geeigneter Stelle zusammen aufbauen

ATEM Mini und Infobeamer vorne + Wandlung auf SDI und HDMI

Kabel zw. Bühne und Regie-Arbeitsplatz:

SDI für Slides zum Encoder (ca. 60 m (teils als zwei Kabel) vorhanden)

Netzwerk (20 + 15 + 10 m vorhanden)

2x XLR Richtung PA (4x 30m (als 20 + 10 m) vorhanden)

Wenn Kameras im Saal vorhanden sind, kann der Encoder auch vorne platziert werden, um sie mit einem der kurzen SDI-Kabel an den Encoder anzuschließen

Kabelstrecken bleiben gleich, weil das Kamerasignal nach vorne muss.

Nicht eingezeichnet:

Strom

Netzwerk-Router aka. WRT, wenn nur wenige Säle oder kein Layer 2/ VLAN zwischen Sälen

Speziallösungen für Audio-Input in die Saalanlage/ PA