decklink-debugger

A tool to probe all inputs of all Blackmagicdesign DeckLink cards in a Linux system, detecting if a signal is present and which image-format it has, showing the results on the terminal and via HTTP on port 8042, allow capturing still images.

Building

See the GitHub project page for instructions how to build the software.

Supported devices

The devices need to support auto configuration. The following list shows which devices are known to be supported by decklink-debugger. Feel free to add new devices to it.

Name	Recognized	Auto detection works	Tested by
Decklink HD Pro	✔	✘	TheAssassin
Intensity Pro	✔	✘	sophie
Decklink Mini Recorder 4k	✔	✔	sophie
Decklink MiniRecorder	✔	✔	MaZderMind
Decklink Duo 2	✔	✔	MaZderMind