Datenspuren 2016

zwei kameras / kamera + grabber

kamera 2 an:

sudo vim /etc/systemd/system/cam2-source.service
Restart = always
sudo systemctl stop bgloop.service
sudo systemctl stop grabber-source.service
sudo systemctl restart cam2-source.service

kamera 2 aus:

sudo vim /etc/systemd/system/cam2-source.service
Restart = no
sudo systemctl stop cam2-source.service
sudo systemctl start bgloop.service
sudo systemctl start grabber-source.service