Tallycoms at Fusion 2018

Intro

At Fusion 2018 we ran a two camera setup for recording only. With the flight cases for room 1 and room 2 came two tallycom's whose config differed from their label and whose config was inconsistent.

Status

device	ipv4	/etc/issue	config
tallycom2-1	10.73.2.15/16	Raspbian GNU/Linux 9	partially ansibilised, please redo completely for next event
tallycom3-2	10.73.2.17/16 (should be 10.73.3.16/16)	Raspbian GNU/Linux 8	partially ansibilised, please redo completely for next event

Sources/Hints

34C4 Tally - Use the tally-pis branch from https://github.com/voc/cm, might need some work and should probably be merged into the master branch eventually.