Audiocase

The Audiocase is our experimental Setup for Conference-Locations, which doesn't have a suitable Audio-System or only have a PA. It consists of a carryable 4HE Case consisting of:

Case:

1x Thon Eco Winkelrack 4 HE mit 19“ Rackaufsteller (http://www.thomann.de/de/thon_lrack_4_he_eco_mit_aufsteller.htm)

1x Thon Rackschublade 2HE (Thon Rackschublade 2HE Rackschublade)

Funkstrecken:

1x Sennheiser XSw 12 Presentation Set E-Band (http://www.thomann.de/de/sennheiser_xsw_12_presentation_set_eband.htm)

1x the t.bone HeadmiKe - D EW (http://www.thomann.de/de/the_tbone_headmike_d_ew.htm)

1x the t.bone Kopfhörer Adapter (http://www.thomann.de/de/akg_kopfhoereradapter_stereoklinke_mini.htm)

2x Sennheiser XSw 65 Vocal Set E-Band (http://www.thomann.de/de/sennheiser_xsw_65_vocal_set_e_band.htm)

1x Sennheiser GAM 3 Rackkit für die XSw Serie (http://www.thomann.de/de/sennheiser_gam_3.htm)

Mischer:

1x QSC TouchMix-8 (http://www.thomann.de/de/qsc_touchmix_8.htm)

1x QSC TMR-1, QSC Touchmix Rack Mount Kit (http://www.thomann.de/de/qsc_tmr_1.htm)

Misc:

1x Equip 333293 19'' Stromverteiler (http://www.thomann.de/de/equip_333293_19_powerbox_sp.htm)

3x the sssnake SK233-05 XLR PATCH (http://www.thomann.de/de/the_sssnake_sk233-06_xlr_patchkabel.htm)

3x Neutrik NC3 MRX, 3 Pol XLR-Male Winkelstecker (http://www.thomann.de/de/neutrik_nc_3_mrx.htm)