Audiocase

more pictures

The Audiocase is our experimental Setup for Conference-Locations, which doesn't have a suitable Audio-System or only have a PA. It consists of a carryable 4HE Case consisting of:

Case:

1x Thon Eco Winkelrack 4 HE mit 19“ Rackaufsteller (http://www.thomann.de/de/thon_lrack_4_he_eco_mit_aufsteller.htm)

1x Thon Rackschublade 2HE (Thon Rackschublade 2HE Rackschublade)

Funkstrecken:

1x Sennheiser XSw 12 Presentation Set E-Band (http://www.thomann.de/de/sennheiser_xsw_12_presentation_set_eband.htm)

1x the t.bone HeadmiKe - D EW (http://www.thomann.de/de/the_tbone_headmike_d_ew.htm)

1x the t.bone Kopfhörer Adapter (http://www.thomann.de/de/akg_kopfhoereradapter_stereoklinke_mini.htm)

2x Sennheiser XSw 65 Vocal Set E-Band (http://www.thomann.de/de/sennheiser_xsw_65_vocal_set_e_band.htm)

1x Sennheiser GAM 3 Rackkit für die XSw Serie (http://www.thomann.de/de/sennheiser_gam_3.htm)

Mischer:

1x QSC TouchMix-8 (http://www.thomann.de/de/qsc_touchmix_8.htm)

1x QSC TMR-1, QSC Touchmix Rack Mount Kit (http://www.thomann.de/de/qsc_tmr_1.htm)

Misc:

1x Equip 333293 19'' Stromverteiler (http://www.thomann.de/de/equip_333293_19_powerbox_sp.htm)

3x the sssnake SK233-05 XLR PATCH (http://www.thomann.de/de/the_sssnake_sk233-06_xlr_patchkabel.htm)

3x Neutrik NC3 MRX, 3 Pol XLR-Male Winkelstecker (http://www.thomann.de/de/neutrik_nc_3_mrx.htm)

Construction

The Case is 4HE height. The uppermost HE is supplied with Hinges, which can fold upwards to easy access to the QSC Touchmix which is mounted on them. On the far end of the Hinges a Power-Distribution bar is mounted which also serves as a handle to lift the Hinges.The 2nd HE contains two of the three XSw Receivers, mounted with a Bracket and connected to the Power Distribution and the QSC Mixer with right-angled XLR Plugs. In the default Setup, the two mounted Receivers are Coupled with the Bodypack-Transmitter and one of the Handheld transmitters.The lower two HEs are filled with a padded Drawer. The Foam inside it has places for two Handheld transmitters, a Bodypack-Transmitter, a third XSw Receiver, a third XLR Cable, a spare Set of Batteries, a Lavalier-Mic and a Headset-Mic.