Flight Cases

This page aims to provide an overview on our flight cases.For details on the content of the cases follow the links below or the Hardware namespace startpage.

Lecture Room Case (S1 to S6)

Currently we have four cases of generation 1 and two of generation 2. They should include everything needed in the lecture rooms. Each part is either labeled or color coded with a cable tie. The current state and constant differences are listed at Hardware status.

Room 1: Green

Room 2: Yellow

Room 3: Blue

Room 4: Red

Room 5: Black

Room 6: White

=== S1 to S4

Content list of the room cases with more photos

Measurements

A single first generation case is (incl. wheels) 102cm wide, 72cm high and has a depth of 54cm.Height without wheels is 57cm. It weighs approximately 60-65kg.

S5+S6

Content list of 2nd generation room cases

Measurements

A single second generation case is (incl. wheels) 104cm wide, 72cm high and has a depth of 54cm.

Height without wheels is 59cm. It weighs approximately TODO

Audio cases (A1, A2, A3, A4)

Content of the audio case

TODO Wie schwer?

A1

LxBxH: 51,5 x 53 x 28 cm

A2

LxBxH: 56 x 53 x 31 cm

A3+A4

LxBxH: 55 x 55 x 40 cm

Regie Box (R)

LxBxH: 60x40x32 cm (Auer-Box)

Contains:

1x HP Ethernet Switch managed, 24+2 ports

1x D-Link Ethernet Switch managed, 24+4 ports

Ethernet set “Regie” in mesh bag DinA2 black

1x 15m

2x 5m

5-10x 3m

5-10x 1.5m

3x misc cables in blue and black (e.g. for uplink)

1x USB 3.0 HDD 2,5“ 2TB in orange mesh bag

1x Viri-Light with power supply

1x Raspberry Pi 1 and power supply

(SDI koax cables with BNC jacks)

misc adapters
* cyber barrier tape, black marker, DinA5 writing pad, pencil

Server case (C)

This case contains hardware that should be placed at the event colo or another well connected place.Measurements (guessed): Length 102cm, width 60cm, height 77cm.

list of servers in the flight case