Flight Cases

This page aims to provide an overview on our flight cases.For details on the content of the cases follow the links below or the Hardware namespace startpage.

Lecture Room Case (S1 to S6)

Currently we have four cases of generation 1 and two of generation 2. They should include everything needed in the lecture rooms. Each part is either labeled or color coded with a cable tie. The current state and constant differences are listed at Hardware status.

Room 1: Green

Room 2: Yellow

Room 3: Blue

Room 4: Red

Room 5: Black

Room 6: White

S1 to S4

A single first generation case is (incl. wheels) 102cm wide, 72cm high and has a depth of 54cm.Height without wheels is 57cm. It weighs approximately 60-65kg. Together with an Audio-Case and an Auer-Box (often shipped together) the weight is ~100-140kg)

Content list of the room cases with more photos

S5 + S6

Content list of 2nd generation room cases

Measurements

A single second generation case is (incl. wheels) 104cm wide, 72cm high and has a depth of 54cm.

Height without wheels is 59cm. It weighs approximately TODO

Spare parts

Wheels: 100mm caster worked well and should be replaced in pairs (eg. Millenium Blue Wheel MkII)

Audio cases (A1, A2, A3, A4, A5, A6)

Content of the audio case

LxBxH: 55 x 55 x 40 cm

Regie Box (R1): SDI over Fibre

LxBxH: 60x40x20 cm (Auer-Box)

Contains:

3x Meshbag Blackmagic Fibre, each containing 2 each Netzteil BM, BM Converter, SDI BNC Module.

Various Fibres

Regie Box (R2): Office

LxBxH: 60x40x32 cm (Auer-Box)

Contains various items to build a voc office:

Ethernet Switch

Ethernet Cables

Schuko Cables and extensions

Various kinds of tape

Phone

USB-HDD

…

See wink for details.