Switch in Colo

VLAN-IDs

Name	Pseudonym	ID
Intern	int	73

Port Konfiguration

Management IP: 10.73.0.253

Port	Vlan	Beschreibung
1	int(t)
2	int(t)
3	int(t)
4	int(t)
5	int (u)
6	int (u)
7	int (u)
8	int (u)
9	int (u)
10	int (u)
11	int (u)
12	int (u)
13	int (u)
14	int (u)
15	int (u)
16	int (u)
17	int (u)
18	int (u)
19	int (u)
20	int (u)
21	int (u)	dual-personality
22	int (u)	dual-personality
23	int (u)	dual-personality
24	int (u)	dual-personality

Configuration dump

; J9145A Configuration Editor; Created on release #W.14.38
hostname "core"
module 1 type J9145A
interface 1
unknown-vlans Disable
exit
interface 2
unknown-vlans Disable
exit
interface 3
unknown-vlans Disable
exit
interface 4
unknown-vlans Disable
exit
interface 5
unknown-vlans Disable
exit
interface 6
unknown-vlans Disable
exit
interface 7
unknown-vlans Disable
exit
interface 8
unknown-vlans Disable
exit
interface 9
unknown-vlans Disable
exit
interface 10
unknown-vlans Disable
exit
interface 11
unknown-vlans Disable
exit
interface 12
unknown-vlans Disable
exit
interface 13
unknown-vlans Disable
exit
interface 14
unknown-vlans Disable
exit
interface 15
unknown-vlans Disable
exit
interface 16
unknown-vlans Disable
exit
interface 17
unknown-vlans Disable
exit
interface 18
unknown-vlans Disable
exit
interface 19
unknown-vlans Disable
exit
interface 20
unknown-vlans Disable
exit
interface 21
unknown-vlans Disable
exit
interface 22
unknown-vlans Disable
exit
interface 23
unknown-vlans Disable
exit
interface 24
unknown-vlans Disable
exit
vlan 1
name "DEFAULT_VLAN"
untagged 1-4
no untagged 5-24
no ip address
exit
vlan 73
name "int"
untagged 5-24
ip address 10.73.0.253 255.255.0.0
tagged 1-4
exit
no web-management
snmp-server community "public" unrestricted
no autorun
password manager