Dr HDMI

https://hdfury.com/product/dr-hdmi/

Specs

Dr. HDMI Technical Specs
HDMI 1.4a compliance
8 EDID banks (5 pre-defined, 2 user programable, 1 copy from Sink device)
Reset HPD-event on the fly !
Up to 50 meters cable loss compensation
Keep source’s HDMI/DVI-D output active
USB upgradable and flashable from computer
User programmable EDID Banks
Sink EDID sniffing feature
Extand signal integrity up to 50 meters !
HDMI Pin14 on/off siwtch to fix HEAC/ARC compatibility issue
Any resolution including HDMI standards
Video Bandwidth : 2.25 Gbps
Video support: Single-link 225Mhz, 2k, WUXGA, 1080p60/12bit deep color and x.v.color
Audio support: Dolby True HD & DTS Master Audio
Input cable equalization
Support extended EDID CEA861, 256 byte
HDCP Pass-Through
Lip Sync Pass-Through
CEC Protocol Pass-Through
Power : Universal USB power adaptor
Compliance: HDCP/FCC/CE
Warranty : 1 year (extendable)
Dimension : 60mm W x 40mm D x 20mm H
Net weight : 50 gramms
Input/Output connector: HDMI female
USB: Mini USB-B female connector

Usage

List of Banks

1. Full, unlimited, all 3D features enabled
2. Full, unlimited, no 3D features
3. 1080i limited – no 3D
4. 720p limited – no 3D
5. 480/576p limited -no 3D
6&7 are special cases which initially hold the same info as #1 but they can be altered with PC software to be anything
8. is the display EDID which can be read by pushing the middle button.
(Once you push the middle button, the contents are read from display and stored to #8 and it is activated)