Event Case Switch(es)

HP ProCurve Switch 2910al-24G, 24-Port (J9145A)

20x 1000BASE-T Ports

4x mini-GBIC transceivers

1x J9008A → 2x SFP+ 10 Ports

Mögliche Erweiterungen:

1x SFP+ J9008A ~700€ (500€ ebay)

HP ProCurve 630 Redundant Power Supply J9443A ~1200€

Install Guide Transceiver Support Matrix new firmware

D-Link SmartPro Switch DGS-1510-28

24x 1000BASE-T Ports

4x SFP+ 10GE

Console Port ⇒ Node

ChassisID: mac 3c:1e:04:9c:0e:a0

Install Guide CLI Guide

Portbelegung

Kursiv geschriebene Belegungen sind alt, können aber z.B. entsprechend wiederverwendet werden.

Port	Vlan	Currently connected to (ifname)	Usage
1	2U	Uplink	Uplink/extern untagged
2	1U 2T	Node ext (live, br-pbl)	Uplink/extern untagged
3	2U	Uplink/extern untagged
4	2U	Uplink/extern untagged
5	1U 2T	Multi-Purpose intern
6	1U 2T	Multi-Purpose intern
7	1U 2T	Multi-Purpose intern
8	1U 2T	Multi-Purpose intern
9	1U 2T	usa int (eth0)	Multi-Purpose intern
10	1U 2T	Multi-Purpose intern
11	1U 2T	Multi-Purpose intern
12	1U 2T	node int (eth, br-int)	Multi-Purpose intern
13	1U	storage (eth0, bond1)	Trunk intern-only
14	1U	storage (eth1, bond1)	Trunk intern-only
15	1U	storage (eth2, bond1)	Trunk intern-only
16	1U	storage (eth3, bond1)	Trunk intern-only
17	1U 2T	RIPE Node	Multi-Purpose intern
18	1U 2T	Multi-Purpose intern
19	1U 2T	Multi-Purpose intern
20	1U	Sun IPMI	intern-only
21	1U	USA IPMI	intern-only
22	1U	fempeg IPMI	intern-only
23	1U	Node IPMI	intern-only
24	1U	Storage IPMI	intern-only
25	1U	Storage 10GE (eth5, bond1)	10GE intern-only
26	Unused	Unused
27	1U <2-4094>T	VOC-Container	all-VLAN-trunk, intern untagged
28	2240T 2241T 3500T 3504T	NOC-Uplink	NOC-Uplink