= HD Capture USB

Very cheap ~10€

Seems to be HDMI ⇒ Composit ⇒ analog video grabber in one device

720×576 is probably the internal resolution video is always 4:3ish

Linux Supported

poor video quality maybe usable for slides

== dmesg / lsusb

[ 58.429473] usb 1-1.2: new high-speed USB device number 4 using ehci-pci
[ 58.541382] usb 1-1.2: config 1 interface 0 altsetting 1 bulk endpoint 0x83 has invalid maxpacket 256
[ 58.544818] usb 1-1.2: New USB device found, idVendor=1b71, idProduct=3002
[ 58.544825] usb 1-1.2: New USB device strings: Mfr=3, Product=4, SerialNumber=2
[ 58.544828] usb 1-1.2: Product: usbtv007
[ 58.544831] usb 1-1.2: Manufacturer: fushicai
[ 58.544834] usb 1-1.2: SerialNumber: 300000000002
[ 58.575954] usbtv 1-1.2:1.0: Fushicai USBTV007 Audio-Video Grabber
[ 58.575991] usbcore: registered new interface driver usbtv

Bus 001 Device 005: ID 1b71:3002 Fushicai USBTV007 Video Grabber [EasyCAP]

== Pictures On the device we received all markings on the ICs where sanded down. Last picture is a capture done with the device