http://jvcpro.de/product/493/gy-hm200e-4kcamhd-live-streaming-camcorder/

Single 1/2.3-inch CMOS image sensor w/12.4M pixels

High quality integrated 12x F1.2-3.5 zoom lens (35mm equivalent: 29.6-355mm)

Dynamic Zoom in HD mode combines optical zoom and pixel mapping to create seamless and lossless 24x zoom

4K Ultra HD recording (150 Mbps) to SDHC/SDXC (UHS-I Speed class 3) cards

4:2:2 Full HD (24-60p) recording at 50Mbps

Live 4K UHD output via HDMI connector

HD-SDI (3G)

Advanced JVC streaming engine compatible with c3voc

2-channel XLR audio inputs with phantom power

IP Network Remote Control, Remote Viewing, Metadata editing, FTP clips

2 position ND filter (1/4, 1/16)

Built-in stereo microphone

Dual SDHC/SDXC slots enable dual backup & continuous recording

3.5-inch colour LCD display (920K pixel) w/smart focus assist

Wired remote control supported

HDMI output (4K output via HDMI only)

0.24-inch colour viewfinder (1.56M pixel) with smart focus assist function

9 user button assignable functions

Includes handle unit, SSL-JVC50 7.4V battery and AC adapter