= Reencoder Te be able to provide video streams to all clients from iPhone to Linux desktops we provide our streams in different resolutions, containers and codecs.

== Speedy & Tweedy

Speedy and Tweedy are to machines build into one 1HE case.

2x Intel Core i7 6700K, 4x 4.00GHz, So.1151, TRAY (CM8066201919901)

2x ASRock Z170M-ITX/ac - Motherboard - Mini-ITX - LGA1151 Socket

2x Corsair Value Select 8GB PC4-17000 - 8 GB - DDR4 - 2133 MHz

2x HGST Ultrastar 7K3000 HUA723020ALA641 - Festplatte - 2TB -

2x Dynatron DYN Kühler K-199 A 1HE

2x Seagate Samsung SpinPoint M9T ST2000LM003 - Festplatte - 2TB -

== Bios Einstellungen

Advanced configuration aktivieren

ACPI Configuration → PCI Devices Power On

Power on failure → enabled