### WORK IN PROGRESS ###

Because of the need of an independent “it-just-works” network, a seperate Flightcase with some Network Hardware is planned.

2x HP JC102A A5820X-24XG-SFP+ Switches for the Core Datasheet

9x HP JC100A A5800 24G Switches for Access Datasheet

The Accessswitches are plannend do screw them in Thomann 1HE Boxes the Core Switches in an 3HE Box together with some cabling stuff.

For the Switches are some well-documented Templates planned, so that nobody needs to configure it by hand.

The Config for the CORE Switches:The Config for the ACCESS Switches:

All Switches run on Comware 5, the documentation for the OS is here: comware_5_cli_guide.pdf

Typical Tasks:

add a user:

on switch side:
system-view
local-user waschtl
password simple 12345678
on your pc:
scp -c aes128-cbc ~/.ssh/id_rsa_1024 waschtl@$switch:/waschtl.key
on switch side:
ssh user waschtl service-type all authentication-type any assign publickey waschtl work-directory flash:/

add a VLAN and allow it on some Interfaces:

system-view
vlan 1337
interface Bridge-Aggregation14
port link-type trunk
port trunk permit vlan 1 3504
interface GigabitEthernet1/0/27
port link-mode bridge
port access vlan 3504

Also planned for the Flightcase (Feature Release):

some long power Cords

long RJ45 Cables

bags with transceivers

some fibers

fiber cleaner

serial cable