= Xnano X5

Annoucement at CNX

SoC – Realtek RTD1295 quad core Cortex-A53 with ARM Mali-T820 MP3 GPU

System Memory – 1GiB

Storage – 16GB eMMC flash + micro SD slot + SATA 3.0

Video Output / Input – HDMI2.0a output up to 4K, HDMI input, AV port

Audio I/O – HDMI Out and In, AV, and optical S/PDIF

Connectivity – 10/100/1000M Ethernet, 802.11ac Wi-Fi, Bluetooth 4.0 with external removable antenna

USB – 1x USB 3.0, 1x USB 2.0 host ports.

Misc – IR receiver, internal Serial Port

Power Supply – 12V/2A

Dimensions – 13.5 x 8.5 x 1.9 cm

Android 6