=melt encoding sniplets

==VOC export profile encoding profile

<consumer pix_fmt="yuv420p" rescale="bilinear" width="1920" aspect="1,77778" top_field_first="2" preset="medium" f="mp4" flags2="-dct8x8" g="13" maxrate="5000k" threads="0" vcodec="libx264" progressive="1" real_time="-3" bf="2" ab="192k" target="/mnt/usb/lnp256_fade2b.mp4" vpre="medium" r="50" height="1080" minrate="100k " acodec="aac" deinterlace_method="yadif" crf="21" ar="48000" vprofile="main" movflags="+faststart" mlt_service="avformat"/>

==group sniplets to uncut.mlt

melt -consumer xml babylon-2018-05-26_21-08-38-22834.ts babylon-2018-05-26_21-11-38-22834.ts > uncut.mlt

==dg50 encoding Direkter encode aus den fuse-ts files

/home/voc/Shotcut.app/melt -progress -track \
/video/datengarten/intros/50.ts \
/opt/crs/fuse/datengarten/hd-capture-2/50/uncut.ts in=1857 out=$((1*60*60*25+3*60*25+52*25)) \
/opt/crs/fuse/datengarten/hd-capture-2/50/uncut.ts in=$((1*60*60*25+18*60*25+2*25)) out=162370 \
/video/datengarten/intros/outro.ts \
-attach-track frei0r.hqdn3d \
-consumer avformat:/video/datengarten/tmp/dg50-out3.mp4 f=mp4 acodec=aac ab=192k \
vcodec=libx264 crf=20 vminrate=100k vmaxrate=5000k vpreset="medium" \
movflags=+faststart bufsize=8192k pix_fmt=yuv420p threads=8

Reencode des fertigen hd.mp4 um die pause herauszuschneiden (pause 1:04:00 → 1:18:11)

melt -progress \
/video/datengarten/tmp/50-hd-camonly.mp4 in=0 out=96000 \
/video/datengarten/tmp/50-hd-camonly.mp4 in=117275 \
-consumer avformat:/home/voc/dg50-out.mp4 f=mp4 acodec=aac ab=192k vcodec=libx264 crf=20\
bufsize=8192k minrate=100k maxrate=5000k vprofile=main vlevel=4.0 movflags=+faststart pix_fmt=yuv420p

==timvideo

xvfb-run -a melt /encode-final/lca2014-intro.dv \
-filter watermark:"/encode-tmp/gentilli/101/101-title.png" \
in=300 out=500 composite.progressive=1 producer.align=centre composite.valign=c composite.halign=c \
/encode-tmp/gentilli/101/start-101.dv \
/encode-tmp/gentilli/101/2014-01-09_15-42-23.dv \
/encode-tmp/gentilli/101/2014-01-09_16-18-04.dv \
/encode-tmp/getilli/101/2014-01-09_16-21-59.dv \
/encode-fin1al/lca2014-exit.dv -consumer avformat

==channel mapping melt ./${file[$i]} $INOUT -profile pal -filter channelcopy to=1 from=0
-consumer avformat:./${output[$i]}.webm progress=1 vb=1000k quality=good deadline=good
deinterlace=1 deinterlace_method=yadif
==melt transcode (fosdem)

#!/bin/bash # # (c) 2013-2015 Holger Levsen holger@layer-acht.org # GPL2 licenced title[0]="Stretching out for trustworthy reproducible builds" speaker[0]="Holger and Lunar" file[0]="k1105_la_fontaine_a_31_142433.mp4" begin_offset[0]="9385" end_offset[0]="17913" videos=1 for i in $(seq 0 $videos) ; do if [ -z "${file[$i]}" ] ; then continue fi if [ -z "${speaker[$i]}" ] ; then echo "${title[$i]} using ${file[$i]}" output[$i]=$(echo ${title[$i]} | sed -s "s# #_#g" ) else echo "${title[$i]} by ${speaker[$i]} using ${file[$i]}" output[$i]=$(echo ${title[$i]} by ${speaker[$i]} | sed -s "s# #_#g" ) fi echo " -> ${output[$i]}" IN="" OUT="" # 25 frames per second if [ ! -z ${begin_offset[$i]} ] ; then IN="in=$(echo ${begin_offset[$i]}*25|bc)" fi if [ ! -z ${end_offset[$i]} ] ; then OUT="out=$(echo ${end_offset[$i]}*25|bc)" fi INOUT="$IN $OUT" echo $INOUT if [ ! -f ./${output[$i]}.webm ] ; then melt ./${file[$i]} $INOUT -profile pal -filter channelcopy to=1 from=0 \ -consumer avformat:./${output[$i]}.webm progress=1 vb=1000k quality=good \ deadline=good deinterlace=1 deinterlace_method=yadif fi done